title example 3.7.9 Bike manufacturing
! Sensitivity analysis
max 12 x1 + 15 x2
subject to 
fin) 20 x1 + 30 x2 < 2400
assem) 15 x1 + 40 x2 < 3000
frames) x1 + x2 < 100
end
leave
